# Ashburn DC2 PoP

```
Sandbox, cage 2020, rack 102
c/o Equinix DC2
21715 Filigree Ct
Ashburn, VA 20147
noc@equinix.com (or ask ERC support@equinix.com folk to escalate to
                 primary on-call NSE)
+1 888 892 0607 equinix 24x7

CURRENT CONTACTS LIST: (2022-05-13)
 Muhammad Waqas Bin Tariq <mwaqas@equinix.com>
 Bheem Lal Nethikar <bnethikar@equinix.com>,
```

## PoP Diagram

![120131.ashburn.jpg](../pics/120131.ashburn.jpg)

## To Do
* Remove akkht.hactrn.net
* Remove cypress.shrubbery.net
* Repurpose serial o0.11 to Cisco ASR r2.iad.rg.net craft port
* Move r2.iad.rg.net MGT ether to an empty port on sw0.iad
* Connect r0.iad to ASR r2.iad to MPLS tunnel Sprint POS to GigE
* Configure r2.iad for Sprint, LAN, ...
* Remove r1.iad (next trip)

## Rack Physical and Wiring

| hostname              | switch        | oob   | oobname | pwr           |  RU  |                           |
| :-------------------- | ------------- | ----- | ------- | ------------- | ---- | ------------------------- |
| r1.iad.rg.net         | s0.f23        | o0.34 | r1      | equinix       |      | Cisco 7206-G1             |
| r2.iad.rg.net         | s0.f23        | o0.34 | r2      | 0.5 & equinix | 9-10 | ASR                       |
| r0.iad.rg.net         | s0.f21        | o0.33 | r0      | equinix       | 7-8  | Juniper MX80              |
| fiber patch panel     |               |       |         |               | 5-6  |                           |
| vm0.iad.rg.net        | s0.02         | o0.10 | vm0     |               | 3    |                           |
| ipmi.vm0.iad.rg.net   | s0.14         |       |         |               | 3    |                           |
| akkht.hactrn.net Eth0 | s0.11         | o0.11 | sra     | 0.1           | 2    | Rob Austein &lt;sra@hactrn.net&gt; |
| akkht.hactrn.net DRAC | s0.12         |       |         |               | 2    | Rob Austein &lt;sra@hactrn.net&gt; |
| o0.iad.rg.net         | s0.01/02      |       |         |               |      | Cisco 2621 (MPC860)       |
| cypress.shrubbery.net | s0.03 & s0.13 | o0.35 | cypress | 0.4           |      | decommissioned 2019.09.20 |
| sw0.iad.rg.net        |               | o0.37 | s0      |               |      | Cisco WS-C3750G-24PS      |
| vm1.iad.rg.net        | s0.06         | o0.38 | srv0    | 0.3           |      |                           |
| emu.machshav.com      | s0.08         | o0.40 | emu     | 0.2           |      | Steven M Bellovin &lt;smb@cs.columbia.edu&gt; |
| emu-2.machshav.com    | s0.09/10      |       |         |               |      | Steven M Bellovin &lt;smb@cs.columbia.edu&gt; |
| pwr0.iad.rg.net       |               | o0.38 | pwr0    | equinix       |      |                           |


* ASR has 2 1gb Fiberstore SFP+ in ports: GE0 && GE1 (see pic below)
* ASR has MGMT Ether plugged into MX80 ge-1/1/7
* Equinix Power Strip aka Leviton
* [photo from 2020.02.18](https://photos.app.goo.gl/aTaqAXH1C14CNbbG8)
 

### Hosts on vm0/1.iad.rg.net / 198.180.150.8/4
```
Node           DTotal DFree MTotal MNode  MFree Pinst Sinst
vm0.iad.rg.net   8.2T  7.4T  78.7G 46.1G  69.8G     4     7
vm1.iad.rg.net   5.4T  4.5T 125.9G 28.8G 108.2G     8     4
```
| Hostname                       | IP Address     | Owner and Email           |
| :----------------------------- | -------------- | ------------------------- |
| bozanicfamily.com              | 198.180.150.5  | Randy Bush &lt;randy@psg.com&gt;      |
| khatovar.hactrn.net            | 198.180.150.30 | Rob Austein &lt;sra@hactrn.net&gt;       |
| m2.macshav.com                 | 198.180.150.45 | Steven M Bellovin &lt;smb@cs.columbia.edu&gt; |
| mail.rg.net                    | 198.180.150.2  | Randy Bush &lt;randy@psg.com&gt;      |
| netsrv.iad.rg.net              | 198.180.150.13 | Randy Bush &lt;randy@psg.com&gt;      |
| pfs0.iad.rg.net                | 198.180.150.3  | Randy Bush &lt;randy@psg.com&gt;      |
| pfs.iad.rg.net                 | 198.180.150.6  | Randy Bush &lt;randy@psg.com&gt;      |
| ran.psg.com                    | 198.180.150.18 | Randy Bush &lt;randy@psg.com&gt;      |
| rgnet.anycast.censurfridns.dk  | 198.180.150.12 | Phil Regnauld &lt;pr@x0.dk&gt;      |
| srv0.iad.rg.net                | 198.180.150.1  | Randy Bush &lt;randy@psg.com&gt;      |
| tor0.iad.rg.net                | 198.180.150.9  | Randy Bush &lt;randy@psg.com&gt;      |
| usbeacon2.iibex.auckland.ac.nz | 198.180.150.52 | Etuate Cocker &lt;ecoc005@aucklanduni.ac.nz&gt; |


 

## vm0.iad.rg.net Hardware

- [Supermicro SYS-6016T-URF with X8DTU-F mobo](http://www.supermicro.com/products/system/1U/6016/SYS-6016T-URF.cfm)
- Power-A&B - UL24-3#24

### vm0.iad.rg.net Disk Configuration
```
vm0.iad.rg.net:/root# tw_cli info

Ctl   Model        (V)Ports  Drives   Units   NotOpt  RRate   VRate  BBU
------------------------------------------------------------------------
c4    9750-4i      4         4        1       0       1       1      -        

vm0.iad.rg.net:/home/randy# tw_cli info c0

Unit  UnitType  Status         %RCmpl  %V/I/M  Stripe  Size(GB)  Cache  AVrfy
------------------------------------------------------------------------------
u0    RAID-5    OK             -       -       256K    8381.87   RiW    ON     

VPort Status         Unit Size      Type  Phy Encl-Slot    Model
------------------------------------------------------------------------------
p0    OK             u0   3.63 TB   SATA  0   -            WDC WD4002FYYZ-01B7 
p1    OK             u0   3.63 TB   SATA  1   -            WD4003FRYZ-01F0DB0
p2    OK             u0   2.73 TB   SATA  2   -            WDC WD3000FYYZ-01UL 
p3    OK             u0   2.73 TB   SATA  3   -            HITACHI HUA723030AL 
```

### vm0.iad.rg.net Disk Drive Serial Numbers

From `smartctl --all -s on -T verypermissive --device=3ware,$i /dev/twl0`
 `smartctl --all --device=3ware,$i /dev/twl0`

| Unit | Model                   | Serial          |
| ---- | ----------------------- | --------------- |
| 0    | WD4002FYYZ-01B7CB1      | K7G9TG6L        |
| 1    | WD4003FRYZ-01F0DB0      | V1JVGGHG 	   |
| 2    | WD3000FYYZ-01UL1B0      | WD-WCC130095709 |
| 3    | HITACHI HUA723030ALA640 | YVHPV0LA        |

* 2022.05.18 replaced p1 WDC WD3000FYYZ-01UL serial WD-WCC130121922

there is a spare 4TB drive in cardboard atop the cisco

## vm1.iad.rg.net Hardware

 **[SuperMicro AS-1022G-URF 2RU Chassis](http://www.supermicro.com/Aplus/system/1U/1022/AS-1022G-URF.cfm)**

- [H8DGU-F Motherboard](http://www.supermicro.com/Aplus/motherboard/Opteron6000/SR56x0/H8DGU-F.cfm)
- [Two AMD Opteron 6344 Abu Dhabi 2.6GHz](http://products.amd.com/en-gb/OpteronCPUDetail.aspx?id=819&f1=&f2=&f3=Yes&f4=&f5=&f6=&f7=&f8=&f9=&f10=&f11=&)
- [Crucial 144G 8 x 16GB 240-Pin DDR3 SDRAM ECC Registered DDR3 1600 (PC3 12800) Server Memory](http://www.crucial.com/usa/en/CT16G3ERSLD4160B?)
- [LSI MegaRAID SATA/SAS 9260-4i 6Gb/s PCI-Express 2.0](http://www.lsi.com/products/raid-controllers/pages/megaraid-sas-9260-4i.aspx)
- [Four Western Digital RE WD3000FYYZ 3TB 7200 RPM 64MB Cache SA T A 6.0Gb/s 3.5" Enterprise Internal Hard Drives](http://wdc.com/en/products/catalog/)

## vm1.iad.rg.net Disk Drives

From `megacli -PDList -aALL | egrep 'Coerced|Inquiry'`

| LUN  | Serial             | Model              | Size     |
| ---- | ------------------ | ------------------ | -------- |
| 0    | WD-WMC130D9JJJZWDC | WD3000FYYZ-01UL1B2 | 2.728 TB |
| 1    | WD-WMC130D1CT76WDC | WD3000FYYZ-01UL1B2 | 2.728 TB |
| 2    | WD-WMC130D2MZFVWDC | WD3000FYYZ-01UL1B2 | 2.728 TB |
| 3    | WD-WMC130D2MZFVWDC | WD3000FYYZ-01UL1B2 | 2.728 TB |


 

## PDU

```
BayTech RPC is accessed via serial from o0.iad.rg.net as pwr0
You will face RPC> prompt.  Type
  CONFIG
  ON x
  OFF x
  REBOOT x

1)...akkht.hactrn.net
2)...emu.machshav.com
3)...srv0.iad.rg.net 
4)...cypress.shrubber
5)...sw0.iad.rg.net  
6)...vm0.iad.rg.net  
```

---

2022.05.18