# Seattle Westin PoP

```
Evocative at KOMO Plaza
140 4th Ave North, Suite 200
Seattle WA 98109
support@evocative.com
+1 888 365-2656 (opt 3 is NOC)
+1 206 290-9206 (on-site tech)

RGnet, LLC.
c/o Lunavi
2001 6th Avenue, Suite 2402
Seattle, WA  98121
Lunavi Support <support@fibercloud.com>
206 777 9988
24x7@ccom.net 206-854-3444 and 206-353-5558

RGnet rack 
  Suite 1809
  Cabinet C2

GreenHouse tie-down to Verio Backbone - Rack 204 Panel 9 Port A6
   r03.sttlwa01.us.bb so-1/1/0

NTT
USID 278679
r05.sttlwa01.us.bb Gi100/0/0/15
WAN IPs on your side:
165.254.106.18/30
2001:418:0:5000::12/126

SIX 1G to USC
RGnet.SW3.SEA eth1/46
RGnet.1809.CAB.C02.P1.1/2
GHD.1809.CAB.D04.P1.M3
GHD.19FMMR.RR.405.3.M3
SIX.19FMMR.RR.506.7.D3

SIX 1G to r1
RGnet.Juniper.Ge-0/0/1
RGnet.1809.CAB.C02.P1.3/4
GHD.1809.CAB.D04.P1.M4
GHD.19FMMR.RR.405.3.M4
SIX.19FMMR.RR.506.7.E3

SIX 10G to Arrcus sixa.rg.net
RGnet.  sixa.rg.net.Ge-0/0/1
RGnet.1809.CAB.C02.P1.5/6
GHD.1809.CAB.D04.P2.F4
GHD.19FMMR.RR.1001.3.F4
SIX.19FMMR.RR.901.9.A4

SprintLink 1G to r1
RGnet.Juniper.Ge-0/0/2
RGnet.1809.CAB.C02.P1.7/8
GHD.1809.CAB.D04.P1.M5
GHD.19FMMR.RR.405.3.M5
Sprint.19FMMR.RR.604.5.A5 (9/10)
```

---

# Westin to KOMO Move

* closing deal with evocative, new colo in komo plaza.

* mike and shaun, the hands on folk from our westin colo, are willing
  to do the heavy lifting of the move if we can schedule it for a
  weekend.  15th or 22nd of april.

* it may take a month or to to get the fiber back to NTT in the westin.

* we will immediately have 10G to SIX across the corridor, and sprint
  is giving us transit across the SIX.  so we will have transit and
  peering on the move.

* we may be able to get vertical power bars from evocative, the new
  colo folk.  they have a ton stashed under the raised floor in santa
  clara, and seem willing to give us enough for the rack.  i am trying
  to see if we can get this in time for joel's next drive to eugene.

## 100mb interfaces on sw0
* atlas probe
* o0.sea.rg.net
* four power bars
* psg.com ipmi
* peering.usc.edu ipmi
* ipmi.vm1.sea.rg.net
* ipmi.vm0.sea.rg.net


---

## Rack Physical and Wiring
Physical Hosts and Wiring

| hostname                      | switch      | ipmi  | oob  | oobname | pwr       | rack  | Model                                                 |
| :---------------------------- | ----------- | ----- | ---- | ------- | --------- | ----- | ----------------------------------------------------- |
| pwr1.sea.rg.net               | s0.16       |       |      |         | 2.x?      | 43    |                                                       |
| sw4.sea.rg.net                | s3.47       |       | 0.08 | sw4     | 1.1       | 41    | Cisco Nexus-3064                                      |
| rcuss0.rg.net                 | s0.23       | N/A   | 0.01 | rcuss0  | 1.2       | 40    | Redstone                                              |
| vm3.sea.rg.net                | s4.20/s4.22 | s4.18 | ???? | vm3     | 0.2       | 39    | SuperMicro SuperServer 6019U-TRT                      |
| r2.sea.rg.net                 | s0.14 s4.36 |       | 0.09 | r2      | 1.7       | 37-38 | Arrcus xxx q2c   aka sixa.rg.net          		   |
| vm4.sea.rg.net                | s4.45/s4.46 | s3.5  | xxxx | xxx     | 1.3       | 36    | Dell 630
| vm2.sea.rg.net                | s0.41/s0.31 | s0.41 | 0.05 | vm2     | 2.7 2.1   | 34-35 | SuperMicro AS-2022G-URF 2RU Chassis                   |
| psg.com                       | s0.13       | s0.19 | 0.02 | psg     | 1.5       | 33    | (see below)                                           |
| seattle01.mux.peering.usc.edu | s0.11 s0.38 | 0.20  |      |         |           | 31    | Supermicro Ethan Katz-Bassett <ethanbkb@gmail.com>    |
| sw3.sea.rg.net                | s0.47       |       | 0.07 | sw3     | 0.7       | 27    | Cisco Nexus-3064                                      |
| sw0.sea.rg.net                | s3.48       |       | 0.06 | sw0     | 0.4       | 26    | Cisco WS-C3750G-POE-48                                |
| pwr2.sea.rg.net               | s0.10       |       |      |         |           | 21    |                                                       |
| atlas0.sea.rg.net             | s0.25       |       |      |         |           | 20.5  |                                                       |
| raid0.sea.rg.net              | s0.27       | s0.03 | ???? | raid0   | 0.6       | 19    | SuperMicro 5018R-WR                                   |
| o0.sea.rg.net                 | s0.06       |       |      |         | 2.4       | 18    | Cyclades ACS-48                                       |
| vm1.sea.rg.net                | s0.34/s0.30 | s0.33 |      | vm1     | 0.2       | 16-17 | (see below)                                           |
| vm0.sea.rg.net                | s0.26/s0.29 | s0.39 | 0.03 | vm0     | 2.5/2.7   | 15    | Supermicro - w/ X7DWU                                 |
| pwr3.sea.rg.net               | s0.18       |       |      |         | x.3       | 13    |                                                       |
| pwr0.sea.rg.net               | s0.12       |       |      |         |           | 11    |                                                       |
| r0.sea.rg.net                 | s0.35/46    |       | 0.11 | r0      | 0.8 & 3.7 | 7     | Cisco ASR1001 commissioned 2018.02.02                 |
| r1.sea.rg.net                 | s0.17       |       | 0.10 | r1      | 2.1 & 3.1 | 5-6   | Juniper M7i                                           |

### Removed
Removed from Rack

| hostname        | switch      | ipmi | oob   | oobname | pwr       | rack  | Model                                 |
| :-------------- | ----------- | ---- | ----- | ------- | --------- | ----- | ------------------------------------- |
| rip.psg.com                   | s4.32  0.04  | rip	 | 1.04      | 36    | NOW VIRT ON VM4  Supermicro 5015M-NTRB w/ Super PDSMU |
| o1.sea.rg.net   | s0.15       |      | 0.04  | o1      | 2.4       | 24    | Cisco 2511                                            |
| dum0.sea.rg.net | s2.23 s2.24 |      | 1.10  | dum0    | 1.1/1.2   | 42    | Supermicro - w/ PDSMi/PDSMA           |
| o0.sea.rg.net                 | s0.05| 1.13  | o0      | 2.6       | 10    | Cisco 2511                                            |
| work1.psg.com   | s1.11       |      | 1.11  | work0   | 3.7       | 39    | decommissioned 2015.07.20             |
| bgp.nu          | s0.07/17    |      |       |         |           | 37-38 | Paul Southworth <pwsouth@gmail.com>           |
| sw2.sea.rg.net  | s0.48       |      | 1.02  | sw2     | 0.7       | 27    | Cisco WS-C3750G-POE                   |
| sw1.sea.rg.net  | s0.01       |      | 1.07  | sw1     | ??        | 25    | SMC SMC8024L2                         |
| r2.sea.rg.net   | s0.14 s2.14 |      | 0.09? | r2      | 2.8       | 7     | Cisco 1001                            |
| r0.sea.rg.net   | s0.03       |      | 0.01  | r0      | 0.1 & 3.4 | 2-4   | Cisco 7206g2 decommisioned 2018.02.02 |



## vm[0-3].sea.rg.net Ganeti Cluster

```
vm4.sea.rg.net:/root# ./do-stat
Node           DTotal DFree MTotal MNode  MFree Pinst Sinst
vm0.sea.rg.net  10.9T  6.9T 125.8G 89.7G  90.2G     9    10
vm1.sea.rg.net   5.9T  2.3T  70.7G 38.1G  53.3G    10    11
vm2.sea.rg.net   5.5T  4.1T  94.4G 23.4G  79.6G     8     5
vm3.sea.rg.net  10.9T  7.1T 503.8G 59.0G 431.3G     3     0
vm4.sea.rg.net   3.6T  2.2T 251.8G 67.0G 234.6G     5     0

Instance              Primary_node   Secondary_Nodes  Disk/0 Memory ConfigVCPUs
adrilankha.hactrn.net vm1.sea.rg.net vm0.sea.rg.net   260.0G   4.0G           1
archive.psg.com       vm1.sea.rg.net vm0.sea.rg.net   200.0G   2.0G           1
atlas9.sea.rg.net     vm1.sea.rg.net                   16.0G   2.0G           1
atlasvm.sea.rg.net    vm1.sea.rg.net                    8.0G   2.0G           1
bbgp.rg.net           vm2.sea.rg.net                   32.0G   2.0G           1
build-u.rpki.net      vm1.sea.rg.net vm2.sea.rg.net   100.0G   1.0G           1
cache0.sea.rpki.net   vm2.sea.rg.net vm0.sea.rg.net   100.0G   2.0G           1
chezrandy.x0.dk       vm2.sea.rg.net                  300.0G   2.0G           1
dataviz.org           vm0.sea.rg.net vm1.sea.rg.net    64.0G   8.0G           1
dnsexp.rg.net         vm2.sea.rg.net                   32.0G   1.0G           1
gogs.rg.net           vm3.sea.rg.net                   65.0G   2.0G           1
hans.rg.net           vm4.sea.rg.net vm0.sea.rg.net   251.0G   4.0G           1
hiroshima.bogus.com   vm1.sea.rg.net vm0.sea.rg.net   250.0G   2.0G           1
jitsi.rg.net          vm1.sea.rg.net vm0.sea.rg.net    32.0G   2.0G           1
mon1.rg.net           vm0.sea.rg.net vm1.sea.rg.net   100.0G   4.0G           1
nagasaki.bogus.com    vm0.sea.rg.net vm1.sea.rg.net   250.0G   4.0G           1
netsrv.sea.rg.net     vm4.sea.rg.net vm1.sea.rg.net   210.0G   1.0G           1
nlring.sea.rg.net     vm2.sea.rg.net vm1.sea.rg.net    32.0G   2.0G           1
okui.psg.com          vm0.sea.rg.net vm1.sea.rg.net  1001.0G   1.0G           1
pfs.sea.rg.net        vm3.sea.rg.net                    8.0G   1.0G           1
pws0                  vm2.sea.rg.net vm1.sea.rg.net   100.0G   4.0G           1
pws1                  vm0.sea.rg.net vm1.sea.rg.net   500.0G   8.0G           1
r1.securerouting.org  vm1.sea.rg.net vm2.sea.rg.net   100.0G   2.0G           1
rcuss-build.rg.net    vm3.sea.rg.net                  316.0G  64.0G          16
rip1.psg.com          vm2.sea.rg.net vm1.sea.rg.net    36.0G   4.0G           1
rip.psg.com           vm4.sea.rg.net vm1.sea.rg.net    32.0G   8.0G           2
shout.rg.net          vm1.sea.rg.net vm0.sea.rg.net    16.0G   1.0G           1
tamias.rg.net         vm0.sea.rg.net vm2.sea.rg.net    17.0G   2.0G           1
turing.sr-ix.com      vm2.sea.rg.net vm0.sea.rg.net   256.0G   2.0G           1
valid.rg.net          vm0.sea.rg.net vm2.sea.rg.net   200.0G   8.0G           1
vault.sea.rg.net      vm4.sea.rg.net vm2.sea.rg.net     8.0G   1.0G           1
work0.psg.com         vm0.sea.rg.net                  200.0G   4.0G           1
xmpp.rg.net           vm1.sea.rg.net vm0.sea.rg.net    33.0G   1.0G           1
zoe.dns.gh            vm4.sea.rg.net vm0.sea.rg.net    32.0G   1.0G           1
zzyzx.sigpipe.org     vm0.sea.rg.net vm1.sea.rg.net   100.0G   2.0G           1
```

isovalent

### BackChannel
net 10, drdb Ports for vm[0-4]

| Switch | Port | Host    | Ether      | IP Address |
| ------ | ---- | ------- | -----      | ---------- |
| sw0    | 29   | vm0.sea | eth1       | 10.0.0.100 |
| sw0    | 30   | vm1.sea | eth5       | 10.0.0.101 |
| sw0    | 31   | vm2.sea | eth1       | 10.0.0.102 |
| sw4    | 22   | vm3.sea | eth1       | 10.0.0.103 |
| sw4    | 46   | vm4.sea | enp130s0f1 | 10.0.0.104 |

### Guest VMs on vm0/1/2/3.sea.rg.net / 147.28.0.14/15/16/29

`gnt-instance list -o "name,pnode,snodes,be/memory,disk.size/0"`

| Instance              | Primary_node   | Secondary_Node | MaxMem | DiskUsage | IP_Address   | SysAdmin                          |
| --------------------- | -------------- | -------------- | ------ | --------- | ------------ | --------------------------------- |
| adrilankha.hactrn.net | vm1.sea.rg.net | vm0.sea.rg.net | 4G     | 260G      | 147.28.0.19  | Rob Austein <sra@hactrn.net>            |
| archive.psg.com       | vm1.sea.rg.net | vm0.sea.rg.net | 1G     | 100G      | 147.28.0.8   | Randy Bush <randy@psg.com>              |
| atlas9.sea.rg.net     | vm1.sea.rg.net |                | 2G     | 16G       | 147.28.0.36  | Randy Bush <randy@psg.com>              |
| atlasvm.sea.rg.net    | vm1.sea.rg.net |                | 2G     | 8G        | 147.28.0.33  | Randy Bush <randy@psg.com>              |
| bbgp.rg.net      	| vm2.sea.rg.net | 		  | 2G     | 32G       | 147.28.0.60  | Randy Bush <randy@psg.com>              |
| build-u.rpki.net      | vm1.sea.rg.net | vm2.sea.rg.net | 1G     | 100G      | 147.28.0.28  | Rob Austein <sra@hactrn.net>            |
| cache0.sea.rpki.net   | vm2.sea.rg.net | vm0.sea.rg.net | 1G     | 100G      | 147.28.0.84  | Randy Bush <randy@psg.com>              |
| chezrandy.x0.dk       | vm2.sea.rg.net |                | 2G     | 200G      | 147.28.0.56  | Phil Regnauld <pr@x0.dk>        	|
| dataviz.org           | vm0.sea.rg.net | vm3sea.rg.net  | 8G     | 64G       | 147.28.0.22  | Randy Bush <randy@psg.com>              |
| gogs.rg.net           | vm3.sea.rg.net | vm2.sea.rg.net | 2G     | 64G       | 147.28.0.10  | Randy Bush <randy@psg.com>              |
| hans.rg.net           | vm0.sea.rg.net | vm2.sea.rg.net | 3G     | 250G      | 147.28.0.42  | Hans Kuhn <hak@flyingpoodle.com>        |
| hiroshima.bogus.com   | vm1.sea.rg.net | vm0.sea.rg.net | 3G     | 250G      | 147.28.0.82  | Hans Kuhn <hak@flyingpoodle.com         |
| jitsi.rg.net          | vm1.sea.rg.net | vm0.sea.rg.net | 2G     | 32G       | 147.28.0.50  | Randy Bush <randy@psg.com>              |
| mon1.rg.net           | vm0.sea.rg.net | vm1.sea.rg.net | 4G     | 100G      | 147.28.0.35  | Randy Bush <randy@psg.com>              |
| nagasaki.bogus.com    | vm0.sea.rg.net | vm1.sea.rg.net | 4G     | 250G      | 147.28.0.81  | Joel Jaeggli <joelja@bogus.com>         |
| netsrv.sea.rg.net     | vm1.sea.rg.net | vm2.sea.rg.net | 1G     | 200G      | 147.28.0.7   | Randy Bush <randy@psg.com>              |
| nlring.sea.rg.net     | vm2.sea.rg.net | vm1.sea.rg.net | 2G     | 32G       | 147.28.0.89  | Randy Bush <randy@psg.com>              |
| okui.psg.com          | vm0.sea.rg.net | vm1.sea.rg.net | 1G     | 1001G     | 147.28.0.25  | Patrick Okui <pokui@psg.com>            |
| pfs.sea.rg.net        | vm3.sea.rg.net |                | 1G     | 8G        | 147.28.0.32  | Randy Bush <randy@psg.com>              |
| pws0                  | vm2.sea.rg.net | vm1.sea.rg.net | 4G     | 100G      | 147.28.0.52  | Paul Southworth <pwsouth@gmail.com>       |
| pws1                  | vm1.sea.rg.net | vm0.sea.rg.net | 8G     | 500G      | 147.28.0.53  | Paul Southworth <pwsouth@gmail.com>       |
| r1.securerouting.org  | vm1.sea.rg.net | vm2.sea.rg.net | 2G     | 100G      | 147.28.0.131 | Sam Weiler <weiler@watson.org>             |
| rcuss-build.rg.net    | vm3.sea.rg.net |  		  | 64G    | 128G      | 147.28.0.170 | Rob Austein <sra@hactrn.net>               |
| rip.psg.com           | vm3.sea.rg.net | vm2.sea.rg.net | 4.0G   | 32.1G     | 147.28.0.39  | Randy Bush <randy@psg.com>              |
| rip1.psg.com          | vm2.sea.rg.net | vm1.sea.rg.net | 1G     | 36G       | 147.28.0.31  | Randy Bush <randy@psg.com>              |
| shout.rg.net          | vm1.sea.rg.net | vm2.sea.rg.net | 1G     | 16G       | 147.28.0.38  | Randy Bush <randy@psg.com>              |
| tamias.rg.net         | vm0.sea.rg.net | vm2.sea.rg.net | 2.0G   | 17.0G     | 147.28.0.80  | Randy Bush <randy@psg.com>              |
| turing.sr-ix.com      | vm2.sea.rg.net | vm3.sea.rg.net | 2G     | 256G      | 147.28.0.17  | Tom Jennings <tom@sr-ix.com>             |
| valid.rg.net          | vm0.sea.rg.net | vm2.sea.rg.net | 8G     | 200G      | 147.28.0.30  | Matthias Wählisch <m.waehlisch@fu-berlin.de> |
| vault.sea.rg.net      | vm3.sea.rg.net | vm2.sea.rg.net | 1G     |   8G      | 147.28.0.2   | Randy Bush <randy@psg.com> |
| work0.psg.com         | vm0.sea.rg.net |  		  | 4G     | 100G      | 147.28.0.11  | Randy Bush <randy@psg.com>              |
| xmpp.rg.net           | vm1.sea.rg.net | vm3.sea.rg.net | 1G     | 34G       | 147.28.0.6   | Randy Bush <randy@psg.com>              |
| zoe.dns.gh            | vm2.sea.rg.net | vm1.sea.rg.net | 1G     | 200G      | 147.28.0.23  | Joel Jaeggli <joelja@bogus.com>           |
| zzyzx.sigpipe.org     | vm0.sea.rg.net | vm1.sea.rg.net | 2G     | 100G      | 147.28.0.13  | Michael Elkins <melkins@sigpipe.org>             |

## vm0.sea.rg.net Hardware

- [SuperMicro SuperServer 6018R-MT Chassis](https://www.supermicro.com/products/system/1u/6018/sys-6018r-mt.cfm)
- [​SuperMicro X10DRL-i MotherBoard](https://www.supermicro.com/products/motherboard/Xeon/C600/X10DRL-i.cfm)

- 2 Intel Xeon E5-2630 V4 2.2 GHz LGA 2011 85W
- 128G Kingston ValueRAM 64GB (4 x 16GB) 288-Pin DDR4 SDRAM ECC  Registered DDR4 2133 (PC4 17000) Server Memory Model KVR21R15D4K4/64

### vm0.sea drives, numbered left to right

From `for i in a b c d; do smartctl -a /dev/sd$i | egrep 'Model|Serial|Capacity'; done`

| Bay  | Model              | Serial   |            |
| ---- | ------------------ | -------- | ---------- |
| 0    | WD6002FFWX-68TZ4N0 | NCGW1TVV | 2016.09.24 |
| 1    | WD6002FFWX-68TZ4N0 | NCGWP5SV | 2016.09.24 |
| 2    | WD6002FFWX-68TZ4N0 | NCGWD6NV | 2016.09.24 |
| 3    | WD6002FFWX-68TZ4N0 | NCGX7MTV | 2016.09.24 |

## vm1.sea.rg.net Hardware

 **[Cisco R210-2121605W - part 74-7341-02 - serial QCI1549A9AY](http://www.cisco.com/en/US/prod/collateral/ps10265/ps10493/data_sheet_c78-587522.html)**

- Effectively: 72GB RAM, 4TB datastore1, 8 cores
- UCS C210 M2 Svr, 2x E5640, 2x4GB, SAS Expand, 1PS
- 2 x 2.66GHz Xeon E5640 80W CPU/12MB cache/DDR3 1066MHz
- 4 x 16GB DDR3-1066MHz RDIMM/PC3-8500/quad rank/Low-Dual Volt
- 2 x 4GB DDR3-1333MHz RDIMM/PC3-10600/dual rank 1Gb DRAMs
- LSI 6G MegaRAID 9261-8i card (RAID 0,1,5,6,10,60) - 512WC
- 8 x 500GB  6Gb SATA  7.2K RPM SFF hot plug/drive sled mounted
- Intel Quad port GbE Controller (E1G44ETG1P20)

### vm1.sea.rg.net Disk Drives

From `megacli -PDList -aALL | egrep 'Coerced|Inquiry'` <br>
 also use `sudo smartctl -a -d sat+megaraid,8  /dev/sda` <br>
 `megacli -PDList -aall | egrep '^(Slot|Firmware)'` is also useful<br>
 `megacli -PDList -aALL | egrep 'Inquiry' | awk '{print $3}' | cut -c1-8`

| LUN  | Serial           | Model       | Size     |
| ---- | --------         | ----------- | -------- |
| 01   | 9XF0VD4E         | ST9500620NS | 464.7 Gb |
| 02   | 9XF21B9B         | ST9500620NS | 464.7 Gb |
| 03   | 9XF0VCK3         | ST9500620NS | 464.7 Gb |
| 04   | 9XF0WE31         | ST9500620NS | 464.7 Gb |
| 05   | 9XF0WEYZ         | ST9500620NS | 464.7 Gb |
| 06   | 9XF0VDFF         | ST9500620NS | 464.7 Gb |
| 07   | 9XF0VBXF         | ST9500620NS | 464.7 Gb |
| 08   | 9XF1YZBY         | ST9500620NS | 464.7 Gb |
| 09   | 9XF0TL1A         | ST9500620NS | 464.7 Gb |
| 10   | 9XF31KKG         | ST9500620NS | 464.7 Gb |
| 11   | 9XF0WDD2         | ST9500620NS | 464.7 Gb |
| 12   | 9XF0VRFD         | ST9500620NS | 464.7 Gb |
| 13   | 9XF21BHB         | ST9500620NS | 464.7 Gb |
| 14   | 9XF0WCVD         | ST9500620NS | 464.7 Gb |
| 15   | 9XF0TQ80         | ST9500620NS | 464.7 Gb |
| 16   | S3Z1NB0M229969T  | ST9500620NS | 464.7 Gb |

Removed:
| 16   | 9XF0VR81         | ST9500620NS | 464.7 Gb | 2022.10.05
| 02   | 9XF0TQ93         | ST9500620NS | 464.7 Gb | 2022.11.17

**[Drive Bays from Cisco Install Manual](https://www.cisco.com/c/en/us/td/docs/unified_computing/ucs/c/hw/C210M1/install/C210M1/replace.html)**

| 	 |        | 	   | 	    |	     |
| ------ | ------ | ------ | ------ | ------ |
|        |        | HDD_01 | HDD_02 | HDD_03 |
|        |        | HDD_04 | HDD_05 | HDD_06 |
| HDD_07 | HDD_08 | HDD_09 | HDD_10 | HDD_11 |
| HDD_12 | HDD_13 | HDD_14 | HDD_15 | HDD_16 |

## vm2.sea.rg.net Hardware

 **[SuperMicro AS-2022G-URF 2RU Chassis](http://www.supermicro.com/Aplus/system/2U/2022/AS-2022G-URF.cfm)**

- [H8DGU-F Motherboard](http://www.supermicro.com/Aplus/motherboard/Opteron6000/SR56x0/H8DGU-F.cfm)
- [Two AMD Opteron 6320 Abu Dhabi 2.8GHz](http://www.amd.com/en-us/products/server/opteron/6000/6300)
- [64GB RAMM as two sets of Kingston 32GB (4 x 8GB) 240-Pin DDR3 SDRAM ECC Unbuffered](http://www.kingston.com/us/memory/search/?partid=KVR16E11K4/32)
- [32G,  two sets of two DIMMs of Crucial Crucial 16GB (2 x 8GB) 240-Pin DDR3  SDRAM ECC Unbuffered DDR3L 1600 (PC3L 12800) Server Memory Model  CT2KIT102472BD160B](http://www.crucial.com/usa/en/ct2kit102472bd160b)
- [LSI MegaRAID SATA/SAS 9260-8i](http://www.lsi.com/products/raid-controllers/pages/megaraid-sas-9260-8i.aspx)
- [Five HGST Ultrastar 7K3000 HUA723020ALA640 (0F12455) 2TB 7200 RPM 64MB Cache SATA 6.0Gb/s](http://www.hgst.com/hard-drives/enterprise-hard-drives/enterprise-sas-drives/ultrastar-7k3000)

### vm2.sea.rg.net Disk Drives

```
vm2.sea.rg.net:/home/randy# megacli -PDList -aALL | egrep '(Slot|^Device Id:|Inquiry)'
Slot Number: 0
Device Id: 11
Inquiry Data:      WD-WCC6N3FVKC2SWDC WD2002FFSX-68PF8N0                  81.00A81
Slot Number: 1
Device Id: 10
Inquiry Data:       MK0251YGKB56HAHitachi HUA723020ALA640                 MK7OAA10
Slot Number: 2
Device Id: 9
Inquiry Data:       MK0251YGKB4N2AHitachi HUA723020ALA640                 MK7OAA10
Slot Number: 3
Device Id: 8
Inquiry Data:       MK0251YGKB58LAHitachi HUA723020ALA640                 MK7OAA10
Slot Number: 4
Device Id: 12
Inquiry Data:       MJ1311YNG6XEVAHitachi HDS5C3030ALA630                 MEAOA5C0


vm2.sea.rg.net:/home/randy# smartctl -a -d sat+megaraid,11  /dev/sda
smartctl 6.6 2016-05-31 r4324 [x86_64-linux-4.9.0-13-amd64] (local build)
Copyright (C) 2002-16, Bruce Allen, Christian Franke, www.smartmontools.org

=== START OF INFORMATION SECTION ===
Device Model:     WDC WD2002FFSX-68PF8N0
Serial Number:    WD-WCC6N3FVKC2S
LU WWN Device Id: 5 0014ee 2687b471f
Firmware Version: 81.00A81
User Capacity:    2,000,398,934,016 bytes [2.00 TB]
Sector Sizes:     512 bytes logical, 4096 bytes physical
Rotation Rate:    7200 rpm
Form Factor:      3.5 inches
Device is:        Not in smartctl database [for details use: -P showall]
ATA Version is:   ACS-3 T13/2161-D revision 5
SATA Version is:  SATA 3.1, 6.0 Gb/s (current: 6.0 Gb/s)
Local Time is:    Thu Aug 19 20:46:26 2021 UTC
SMART support is: Available - device has SMART capability.
SMART support is: Enabled

```

| LUN  | Serial          | Model              | Size     |
| ---- | --------------- | ------------------ | -------- |
| 0    | WCC6N3FVKC2S    | WD2002FFSX-68PF8N0 | 1.818 TB |
| 1    | MK0251YGKB56HA  | MK7OAA10 	      | 1.818 TB |
| 2    | MK0251YGKB4N2A  | MK7OAA10 	      | 1.818 TB |
| 3    | MK0251YGKB58LA  | MK7OAA10 	      | 1.818 TB |
| 4    | MJ1311YNG6XEVA  | MEAOA5C0 	      | 2.728 TB |

2021.08.19 LUN0 drive MK0171YFK3TVGA removed

## vm3.sea.rg.net Hardware

 **[SuperMicro SuperServer 6019U-TRT](https://www.supermicro.com/products/system/1U/6019/SYS-6019U-TRT.cfm)**

- [X10DRW-iT Motherboard](https://www.supermicro.com/products/motherboard/Xeon/C600/X10DRW-IT.cfm)
- [Two Intel Ten Core 2.4Ghz Xeon 25MB cache 8.0GT/s QPI (90W) (E5-2640v4)](http://ark.intel.com/products/92984/Intel-Xeon-Processor-E5-2640-v4-25M-Cache-2_40-GHz)
- 128G RAM - 8x16GB DDR4 2400Mhz 19200 ECC/REG
- [Four HGST 6TB Enterprise SATA3 6Gb/s 7200RPM 128MB](https://www.hgst.com/products/hard-drives/ultrastar-7k6000)

### vm3.sea drives, we guess numbered left to right

From `for i in a b c d; do smartctl -a /dev/sd$i | egrep 'Model|Serial|Capacity'; done`

| Bay  | Model                | Serial         | Capacity | Installed  |
| ---- | -------------------- | -------------- | -------- | ---------- |
| 0    | HGST HUS726060ALE610 | K1J48AGD       | 6TB      | 2017.08.17 |
| 1    | HGST HUS726060ALE610 | K1J2PTND       | 6TB      | 2017.08.17 | bad
| 2    | HGST HUS726060ALE610 | K8J6HV2N       | 6TB      | 2022.09.15 |
| 3    | HGST HUS726060ALE610 | K1J46RHD       | 6TB      | 2017.08.17 |

replaced:
| 2    | HGST HUS726060ALA640 | AR11001EV17LLB | 6TB      | 2022.09.15 |
```

for i in b c d e; do echo $i; smartctl -a /dev/sd$i | egrep '(^Serial|Extended)'; done

## psg.com

[SUPERMICRO AS-1012G-MTF 1U Rackmount](http://www.supermicro.com/Aplus/system/1U/1012/AS-1012G-MTF.cfm) [H8SGL-F mobo](http://www.supermicro.com/Aplus/motherboard/Opteron6000/SR56x0/H8SGL-F.cfm)

From `for i in 0 1 2 3 4; do smartctl -a /dev/ada$i | egrep 'Model|Serial|Capacity'; done`

| LUN  | Model                  | Serial          | Size |
| ---- | ---------------------- | --------------- | ---- |
| 0    | WDC WD2000F9YZ-09N20L0 | WD-WCC1P0469969 | 2TB  |
| 1    | WDC WD2005FBYZ-01YCBB1 | WD-WMC6N0F1F8SD | 2TB  |

WDC WD2000F9YZ-09N20L0  WD-WCC1P0648270 removed from ata1 2017.04.09

WD-WCC1P0654846 replaced on 2017.03.04

## vm4.sea.rg.net Hardware

- Dell Poweredge R630 Server 2xE5-2640V4 10-core 2.4GHz, 256GB RAM, H730
- Service tag: 6TL7MN2
- Express Service Code 14849840990
- [How to configure the DELL PERC H700/H710/H730/H730P RAID controller](https://www.scaleway.com/en/docs/dedibox/hardware/how-to/configure-dell-perc-h700/)


## raid0.sea.rg.net

- [5018R-WR Chassis + MoBo](https://www.supermicro.com/products/system/1u/5018/sys-5018r-wr.cfm)
- [X10SRW-F Motherboard](https://www.supermicro.com/products/motherboard/Xeon/C600/X10SRW-F.cfm)
- [Intel Xeon® Processor E5-2609 v4](https://ark.intel.com/products/92990/Intel-Xeon-Processor-E5-2609-v4-20M-Cache-1-70-GHz-)
- Samsung DDR4 2133MHzCL15 16GB RegECC 2Rx4 (PC4 2133) Internal Memory M393A2G40DB0-CPB
- FreeBSD USB key left in USB port


### raid0.sea.rg.net Drive Bays

 From `for i in {0..3}; do smartctl -a /dev/ada$i | egrep 'Model|Serial|Capacity'; done`

| LUN  | Model                | Serial          | Capacity | Date       |
| ---- | -------------------- | --------------- | -------- | ---------- |
| 0    | WDC WD60EFRX-68L0BN1 | WD-WX41DA5F88N9 | 6tb      | 2018.12.09 |
| 1    | WDC WD60EFRX-68L0BN1 | WD-WX11D363T2Y5 | 6tb      | 2018.12.09 |
| 2    | WDC WD60EFRX-68L0BN1 | WD-WX11D3678XTL | 6tb      | 2018.12.09 |
| 3    | WDC WD60EFRX-68L0BN1 | WD-WX41D75LN9KC | 6tb      | 2018.12.09 |

## rip.psg.com

[PDSMU with a Xeon and 4GB RAM](http://www.supermicro.com/products/motherboard/Xeon3000/3010/PDSMU.cfm)

| LUN  | Serial          | Model                           | Size |
| ---- | --------------- | ------------------------------- | ---- |
| 0    | 9QE7MXMC        | ST3250820NS                     | 250G |
| 1    | WD-WMC5C0D5MXU1 | WDC WD2000F9YZ-09N20L1 01.01A02 | 2TB  |
| 2    | 9QE7MY84        | ST3250820NS                     | 250G |
| 3    | WD-WMC5C0E2C2L0 | WDC WD2000F9YZ-09N20L1 01.01A02 | 2TB  |

## Switches

| name           | mfr   | model                | ip sddress   |
| -------------- | ----- | -------------------- | ------------ |
| sw0.sea.rg.net | Cisco | WS-C3750G-48PS       | 147.28.0.253 |
| sw3.sea.rg.net | Cisco | Nexus3064 48x10GE +4 | 147.28.0.239 |
| sw4.sea.rg.net | Cisco | Nexus3064 48x10GE +4 | 147.28.0.238 |

### Remoived

| sw1.sea.rg.net | SMC   | SMC8024L2      | 147.28.0.252 |
| -------------- | ----- | -------------- | ------------ |
| sw2.sea.rg.net | Cisco | WS-C3750G-24PS | 147.28.0.246 |

## Miscelaneous Data

### Spare Drives

|                  |              |          |      |
| ---------------- | ------------ | -------- | ---- |
| spares in westin |              |          |      |
|                  |              |          |      |
| HGST             | H3D30003254S | YNG1E3ZC | 3TB  |
| Seagate          | ST31000528AS | 6VPCVN1Y | 1TB  |
| Seagate          | ST3750640A8  | 3QD06D5B | 750G |
| HGST             | 118032816    | YFJLBZ5A | 2TB  |
|                  |              |          |      |

### r1.sea gigether pic left to right

|        |           |
| ------ | --------- |
| LAN    | copper    |
| unused | copper    |
| six    | copper    |
| unused | fiber sfp |
|        |           |

```
Westin NTT/Verio 100baseFX
PSG-STTLWA01-FE-VDR001 (199.238.113.9)
r05.sttlwa01.us.bb.gin.ntt.net.
1000 LX
Westin NTT/Verio OC3
PSG-STTLWA01-OC3-VDR001 (129.250.11.41)
r02.sttlwa01.us.bb.gin.ntt.net
SM IR
```

FastEthernet5/6 is up, line protocol is up (connected)

Hardware is C6k 100Mb 802.3, address is 00d0.0135.840a (bia 00d0.0135.840a) Description: AX: PSG - local wire

Westin OC3c sprint facility # 10038527

SprintLink noc 800-232-6895  \
<noc@sprint.net>

FiberCloud tie-down to Sprint in MMR - Rack 303 Panel 1 Port L2 Single Mode 

## Router Topology

[![200511.westin.jpg](../pics/200511.westin.jpg)]
 

## New Switching

[![180802.arrcus-sea.jpg](../pics/180802.arrcus-sea.jpg)]

---

2023.04.10
