# Dallas Google PoP

## New Google POP

```
Site DFW 28
Cage 4000.40
1950 N Stemmons Freeway
Suite 4000
Dallas, TX 75207

Racks 4-11 4-12
  RGnet in 4-12
  IETF/Deadalus/RGnet in 4-11

Shipping Address:
 Google - chris morrow
 c/o: Infomart Suite 4000
 1950 N Stemmons Freeway
 Dallas, TX 75207
```

## Hardware Inventory
```
r1 Juniper MX240
r2 cisco 9001
sw0 cisco 2960G-48TC-L with fiber to 12406
sw2 Nexus3064 48x10GE
sw3 Nexus3064 48x10GE
o2 Cyclades® ACS Advanced Console Server
pwr0 Servertech Horizontal Power Strip (8port) Part Number: CW-8H2-C20
pwr1 Servertech Horizontal Power Strip (8port) Part Number: CW-8H2-C20

Removed
dfw0 1ru compute server SuperMicro SYS-6015W-NTRB w/ X7DWU
dfw1 3ru big raid server SuperMicro CSE-836TQ-R800B w/ X7SBE
dfw2 2ru Junosphere virtualization server
```

---

## Rack Physical and Wiring

| hostname                     | switch               | ipmi         | oob     | oobname    | pwr                        | rack    |                    |
| :--------------------------- | ---------------------| ------------ | ------- | ---------- | ---------------------------| ------- | -------------------|
| o2.dfw.rg.net                | sw0.35               |              | 1.8     | o2         |                            |         | Cyclades® ACS-48   |
| [equnix IX fiber]            | 0.46                 |              |         |            |                            |         |                    |
| r1.dfw.rg.net.2/2/0          | 0.07                 |              | 2.15    | r1         |                            | 0.13-17 |  LAN               |
| r1.dfw.rg.net.2/2/1          | 2.03                 |              | 2.15    | r2         |                            | 0.13-17 |  NTT (VLAN 53)     |
| r2.dfw.rg.net-0/0/1/0        | 2.05                 | 0.08         | 2.3     | r2         |                            | 0.18.19 |  NTT VLAN 50       |
| r2.dfw.rg.net.0/1/1          | 2.06                 |              | 2.3     |            |                            | 0.18.19 |  LAN               |
| o1.dfw.rg.net                | 0.40                 |              | 0.aux   |            | 1.1                        | 0.22-23 |                    |
| sw0.dfw.rg.net               | 2.47                 |              | 2.13    | sw0        | [^1]                       | 0.28    |                    |
| sw2.dfw.rg.net               | 0.47                 |              | 2.02    | sw2        | [^1]                       | 0.30    |                    |
| raid0.dfw.rg.net             | [^2]                 | 2.18         | 2.44    | raid0      | 0.5/1.5                    | 0.36-38 |                    |
| vm0.dfx.rg.net               | 2.27  2.25(drbd)     | 2.20         | 2.5     | vm0.dfx    | pwr0b B1-9  pwr0r B1-9     | 0.40    |                    |
| vm1.dfx.rg.net               | 2.28  2.26(drbd)     | 2.19         | 2.6     | vm1.dfx    | pwr0b B1-10 pwr0r B1-10    | 0.41    |                    |
| atlas.dfw.rg.net             | 0.33                 |              |         |            | vm1.dfx USB                |         |                    |
| b0.noc.ietf.org              | 3.32                 | 3.31         | 2.45    | b0         | 0.4/1.4                    | 1.26    |                    |
| sw3.dfw.rg.net               | 2.48                 |              | 2.30    | sw3        | 0.4/1.4                    | 1.30    |                    |
| dallas01.mux.peering.usc.edu | 0.38                 |              | 2.46    | usc        | 0.7/1.7                    | 1.40    |                    |
| rtcolo.daedalus.com          |                      | xx           | 2.45    | b0         | xx                         | 1.41    |                    |
| paddington.richosman         | 0.22                 |              | 2.47    | paddington | 0.8/1.8                    | 1.42    |                    |
| kingsx.richosman.com         | 0.21                 |              | 2.48    | kingsx     | 0.6/1.6                    | 1.43-44 |                    |
| pwr1.red.dfw.rg.net          | 0.41                 |              | 2.9     | pwr1-red   | subfl                      | 26      |                    |
| pwr1.blue.dfw.rg.net         | 0.41                 |              | 2.10    | pwr1-blue  | subfl                      | 26      |                    |
| pwr0-blue.dfw.rg.net         | 0.42                 |              | 2.16    | pwr0-blue  | subfl                      | -       |                    |
| pwr0-red.dfw.rg.net          | 0.42                 |              | 2.17    | pwr0-red   | subfl                      | -       |                    |

[^1]: vm servers' ethers are connected to sw2.dfw as follows:

| vm   | ipmi   | e0     | e1     |
| ---- | ------ | ------ | ------ |
| vm0  | sw2-20 | sw2-25 | sw2-26 |
| vm1  | sw2-19 | sw2-27 | sw2-28 |

[^2]: raid0 ethers are connected to sw2.dfw as follows:

| ipmi   | e0     | e1     | 10g 0  | 10g 1  |
| ------ | ------ | ------ | ------ | ------ |
| sw2-32 | sw2-16 | sw2-17 | sw2-29 | sw2-30 |


## Ganeti Cluster / 198.180.152.30 / 198.180.152.7

```
Node           DTotal DFree MTotal MNode  MFree Pinst Sinst
vm0.dfx.rg.net   3.1T  1.6T 251.8G 41.0G 237.2G     7     4
vm1.dfx.rg.net   3.1T  2.0T 251.8G  4.7G 246.4G     5     6

Instance           Primary_node   Secondary_Nodes Disk/0 Memory
ca.rg.net          vm0.dfx.rg.net vm1.dfx.rg.net  128.0G   4.0G
cu0.dfw.rg.net     vm1.dfx.rg.net vm0.dfx.rg.net   12.0G   512M
git.rg.net         vm0.dfx.rg.net vm1.dfx.rg.net   32.0G   2.0G
icir.dfw.rg.net    vm0.dfx.rg.net vm1.dfx.rg.net  400.0G   8.0G
mail.rg.net        vm1.dfx.rg.net vm0.dfx.rg.net   12.0G   1.0G
mon0.rg.net        vm1.dfx.rg.net vm0.dfx.rg.net  150.0G  16.0G
netsrv.dfw.rg.net  vm0.dfx.rg.net vm1.dfx.rg.net  100.0G   1.0G
nms.rg.net         vm0.dfx.rg.net vm1.dfx.rg.net   80.0G   2.0G
petunia.hactrn.net vm0.dfx.rg.net vm1.dfx.rg.net  120.0G   6.0G
wireguard.rg.net   vm0.dfx.rg.net                  10.0G   2.0G
wp.rg.net          vm1.dfx.rg.net                  64.0G   4.0G
ymbk.com           vm1.dfx.rg.net vm0.dfx.rg.net   16.0G   512M
```

## vm0.dfx.rg.net vm1.dfx.rg.net
VMs are [Supermicro A+ Server 1114S-WTRT Systems](https://www.supermicro.com/Aplus/system/1U/1114/AS-1114S-WTRT.cfm)<br>
With [Supermicro H12SSW-NT Motherboards](https://www.supermicro.com/en/products/motherboard/H12SSW-NT)<br>
With one AMD EPYCTM 7443P Single Socket Processor 24-Core 2.85GHz<br>
With 256G of RAM each<br>
And 2 Samsung 250GB 970 EVO+ Series - M.2 NVMe PCIe (<1DWPD) (MZ-V7S250B)<br>
And 8 Samsung 960GB 883 DCT Series - 2.5" SSD SATA 6Gb/s (<1DWPD)
(MZ-7LH960NE)<br>
Serial Numbers: iX1210A-IXN S/N's A1-86827 and A1-86828<br>

### vm[0-1].dfx.rg.net Disk Drives

```
vm0.dfx.rg.net:/home/randy# for i in a b c d e f g h; do echo -n "sd$i "; smartctl -a /dev/sd$i | egrep "Serial|Model"; done
sda Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R316039
sdb Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R107119
sdc Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R316036
sdd Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R316032
sde Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R303811
sdf Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R316042
sdg Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R107124
sdh Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R316040

vm1.dfx.rg.net:/home/randy#  for i in a b c d e f g h; do echo -n "sd$i "; smartctl -a /dev/sd$i | egrep "Serial|Model"; done
sda Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R316035
sdb Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R303827
sdc Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R316034
sdd Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R303829
sde Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R303777
sdf Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R303803
sdg Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R303764
sdh Device Model:     SAMSUNG MZ7LH960HAJR-00005
Serial Number:    S45NNA0R316031
```

## Hosts on vm0/1.dfx.rg.net

| Instance            | Primary_node   | Secondary_Node | MaxMem | DiskUsage | IP_Address      | SysAdmin                                   |
| ------------------- | -------------- | -------------- | ------ | --------- | --------------- | ------------------------------------------ |
| ca.rg.net           | vm0.dfw.rg.net | vm1.dfw.rg.net | 4.0G   | 128.0G    | 198.180.152.6   | Randy Bush &lt;randy@psg.com&gt;                 |
| cu0.dfw.rg.net      | vm1.dfw.rg.net | vm0.dfw.rg.net | 512M   | 12.0G     | 198.180.152.71  | Steven M Bellovin &lt;smb@cs.columbia.edu&gt; John Koh &lt;koh@…&gt; |
| git.rg.net          | vm0.dfw.rg.net | vm1.dfw.rg.net | 2.0G   | 34.0G     | 198.180.152.8   | Randy Bush &lt;randy@psg.com&gt;                 |
| icir.dfw.rg.net     | vm0.dfw.rg.net | vm1.dfw.rg.net | 1.0G   | 32.0G     | 198.180.152.57  | Bill Marczak &lt;billmar@gmail.com&gt;           |
| mail.rg.net 	      | vm0.dfw.rg.net | vm1.dfw.rg.net | 2.0G	 | 12.0G     | 198.180.152.11  | Randy Bush &lt;randy@psg.com&gt;     	    |
| mon0.rg.net 	      | vm1.dfw.rg.net | vm0.dfw.rg.net | 16G    | 150.1G    | 198.180.152.62  | Randy Bush &lt;randy@psg.com&gt;		    |
| netsrv.dfw.rg.net   | vm0.dfw.rg.net | vm1.dfw.rg.net | 1.0G   | 100G      | 198.180.152.15  | Randy Bush &lt;randy@psg.com&gt;                 |
| nms.rg.net          | vm0.dfw.rg.net | vm1.dfw.rg.net | 2.0G   | 20G       | 198.180.152.9   | Randy Bush &lt;randy@psg.com&gt;                 |
| petunia.hactrn.net  | vm0.dfw.rg,net | vm1.dfw.rg.net | 6G     | 120G      | 198.180.152.200 | Rob Austein &lt;sra@hactrn.net&gt;               |
| wireguard.rg.net    | vm0.dfw.rg.net | 		| 4G	 | 64G	     | 198.180.152.16  | Hans Kuhn &lt;hans@flyingpoodle.com&gt;	    |
| wp.rg.net	      | vm1.dfw.rg.net | 		| 2G	 | 10G	     | 198.180.152.56  | Randy Bush &lt;randy@psg.com&gt;		    |
| ymbk.com            | vm1.dfw.rg.net | vm0.dfw.rg.net | 512M   | 16.1G     | 198.180.152.10  | Randy Bush &lt;randy@psg.com&gt;                 |


## raid0.dfw.rg.net

Dell R530<br>
Service Tag: HQWPW52<br>
PERC H730P RAID Controller, 2G B NV Cache, Mini card<br>
2 x 4TB in md0 RAID1 as opsys<br>
5 x 16TB in zfs<br>
[System Configuration Page](https://www.dell.com/support/home/en-us/product-support/servicetag/0-V1RMSUVWMzFWOUdxdk5Va1doY2oyQT090/overview)

### raid0 Drives

`smartctl -a -d megaraid,[0-7] /dev/bus/0`<br>
Look for smart scan errors with `for i in 0 1 2 3 4 5 6 7; do echo -n "$i  "; smctl -a -d megaraid,$i /dev/bus/0 | grep 'Completed with'; echo; done`

|     |                 |                      |          |             |
| --- | --------------- | -------------------- | -------- | ----------- |
| Bay | Manufacturer    | Model                | Serial   | Installed   | 
| 0   | Seagate         | ST4000NM0005         | Z4C056TC | 2022.06.06  |
| 1   | Seagate         | ST4000NM0005         | Z4C056KT | 2022.06.06  |
| 2   | Western Digital | WD161KRYZ-01AGBB0    | 2PH9PMWT | 2022.06.06  |
| 3   | Western Digital | WD161KRYZ-01AGBB0    | 2PHA0RMT | 2022.06.06  |
| 4   | Western Digital | WD161KRYZ-01AGBB0    | 2PH9NJNT | 2022.06.06  |
| 5   | Western Digital | WD161KRYZ-01AGBB0    | 2PH69HJJ | 2022.06.06  |
| 6   | Seagate	        | ST16000NM000J-2TW103 | ZR706BX0 | 2022.06.06  |

--------

## Disgusting Details
```
Power
    SO1-A:5C2.2-62/64
    SO2-A:5C2.2-66/68
    SO1-B:5D2.2-62/64
    SO2-B:5D2.2-66/68
    C-Side is Blue and that = "A" feed
    D-Side is Yellow and that = "B" feed
    [ SO2-B:5D2.2-66/68 will not be used ]

The demarc for the xconnects is as follows:
    pp01.dfw06
    137-138 M3 Future
    139-140 M4 Future
    141-142 M5 Equinix IX Cable ID #20466027 Terminated on CP:0104:1068601 ports 3/4
    143-144 M6 NTT/Verio r08.dllstx09.us.bb g0/6/0/29

Rge Equinix order info for the exchange fiber:
Ordering contact- Chris Morrow and/or CSM- Shazyra Irizarry
Technical contact – Randy Bush  <randy@psg.com>
IBX- DA1
Order:  1-97362053795
WOA-    3-97445043133 (IX Port Install)
WOA-    3-97448754941 (NCC Cable install)
Serial # 20466027 ; terminated on CP:0104:1068601 ports 3/4

---

Dallas Equinix Colo, Downstairs

Google demarc for the riser cable on the Equinix end is Suite 1034 Cage
00372 Cabinet 105

NTT/Verio TDI
Cage 220, Cab 101 FP#1, Port NA, SMF/SC.
r08.dllstx09.us.bb g0/6/0/29

Media: MMF
Connector: SC

---  ntt circuit ---

EQUINIX INC. - Cross Connect Order Complete - 817885.1.1.2
Completed On: 08-JUN-2009
IBX: DA1
Type of Order: Cross Connect
Cage: DA1::00080:EQUINIX.COM
Cabinet Number: 0101
A-Side Patch Panel/Module/Port: PP:0105:2288||1
Z-Side Customer and Cage Number: YOUTUBE, LLC     
     DA1::00372:YOUTUBE
Z-Side Cabinet Number: 0105
Carrier Circuit ID(if applicable): EQUINIX SANDBOX
Z-Side Patch Panel/Module/Port: VP:0105:69862||143
Cable ID: 1234912

EQUINIX INC. - Cross Connect Order Complete - 817885.2.1.2
Completed On: 05-JUN-2009
IBX: DA1
Type of Order: Cross Connect
Cage: DA1::00080:EQUINIX.COM
Cabinet Number: 0101
A-Side Patch Panel/Module/Port: PP:0105:74459||3
Z-Side Customer and Cage Number: NTT AMERICA, INC.
     DA1::00220:NTT AMERICA, INC. (Verio)
Z-Side Cabinet Number: 0101
Carrier Circuit ID(if applicable): EQUINIX SANDBOX
Z-Side Patch Panel/Module/Port: PP:0101:2375||15
Cable ID: 1234913

For both crossconnects, even though the "Cabinet Number" field shows
"0101", the actual Equinix A-Side cab is "0105" as listed in the panel
info.  And to reduce cabling and points of failure, the IBX site
technicians said that they would be connecting both crossconnects
directly into each other rather than with an intermediate patch cable.

--- equinix exchange ---

csw7.da1, gig 0/35, Sandbox/RGNet, IX, circuit id 1236454
```

## Routers

[![120131.dallas-routers.jpg](../pics/120131.dallas-routers.jpg)]

## Tapping BGP Feeds

[![110617.dfw-data-tap.jpg](../pics/110617.dfw-data-tap.jpg)]


## Old Google PoP

We were in Google POP in Via West

```
Viawest/Dataside
1950 Stemmons Freeway, Suite 2033
Dallas TX 75027
+1-214-231-0162
Mark for "inside delivery"

Google PoP DFW06
Rack Location: 6.3
Rack: ESW E-00589-01, Black Caster and Mounting Rails, No Door, 7Ft.
```

---

## Devices Removed

| hostname                     | switch               | ipmi         | oob     | oobname    | pwr                        | rack  |                                       |
| :--------------------------- | ---------------------| ------------ | ------- | ---------- | ---------------------------| ----- | ------------------------------------- |
| r0.dfw.rg.net-rp0            | 0.45                 |              | 0.01    | r00        | subfl                      | 03-13 |                                       |
| r0.dfw.rg.net-rp0mgt         | 0.33                 |              |         |            |                            | 03-13 |                                       |
| r0.dfw.rg.net-rp1            | 0.??                 |              | 0.02    | r01        |                            | 03-13 |                                       |
| r0.dfw.rg.net-rp1mgt         | 0.34                 |              |         |            |                            | 03-13 |                                       |
| [r0.2/0/4 LAN]               | 0.04                 |              |         |            |                            | 03-13 |                                       |
| [r0.2/0/5 ntt fiber]         | 0.05                 |              |         |            |                            | 03-13 |                                       |
| [r0.2/0/6 spare]             | 0.06                 |              |         |            |                            | 03-13 |                                       |
| [r0.2/0/7 equinix ix]        | 0.15                 |              |         |            |                            | 03-13 |                                       |
| sw1.dfw.rg.net               |                      |              | 0.13    | sw1        | [^1]                       | 0.35  |                                       |

[^2]: PTSS/B is connected to power 0.2/1.2 and controls both sw0 and sw1 



## DEAD raid0.dfw.rg.net

[Mobo Supermicro X7SB4/E](https://www.supermicro.com/products/motherboard/Xeon3000/3210/X7SB4.cfm) [IPMI AOC-IPMI20-E](http://www.supermicro.com/products/accessories/addon/AOC-IPMI20-E.cfm)

### raid0 disk drive physical order markings on drive carriers

|      |      |      |      |
| ---- | ---- | ---- | ---- |
| 00   | 10   | 20   | 30   |
| 01   | 11   | 21   | 31   |
| 02   | 12   | 22   | 32   |
| 03   | 13   | 23   | 33   |


```
for i in 1 2 3 4 5 6 7 8 9 10 11 12 13 14 15 16; do
   echo -n "1/$i  ";
   smartctl -i -d hpt,1/$i /dev/hptrr | grep ^Serial;
   done
```
1/1  Serial Number:    WD-WMAZA9378538
1/2  Serial Number:    V1KVXSXG
1/3  Serial Number:    YGGU1YTA
1/4  Serial Number:    WD-WMAZA9520754
1/5  Serial Number:    WD-WCAVY0114154
1/6  Serial Number:    WD-WMC5C0D9L6HV
1/7  Serial Number:    WD-WCC6N5UY8H5P
1/8  Serial Number:    WD-WCC300759632
1/9  Serial Number:    WD-WCC6N6DDJ7DT
1/10  Serial Number:    WD-WCC6N6VTE2NF
1/11  Serial Number:    WD-WMC5C0D8Z7FV
1/12  Serial Number:    WD-WMC6N0J6S9AV
1/13  Serial Number:    WD-WCC4MLULA4S4
1/14  Serial Number:    WD-WMC6N0F8FU0U
1/15  Serial Number:    WD-WCAVY0090692
1/16  Serial Number:    WD-WCC6N5CLHYSS

| Bay  | ID   | Drive | Name      | Serial Number   |
| ---- | ---- | ----- | --------- | --------------- |
| 20   | 1/1  | da0   | JBOD-1-1  | WD-WMAZA9378538 |
| 21   | 1/2  | da1   | JBOD-1-2  | V1KVXSXG        |
| 22   | 1/3  | da2   | JBOD-1-3  | WD-WCC300755734 |
| 23   | 1/4  | da3   | JBOD-1-4  | WD-WMAZA9520754 |
| 00   | 1/5  | da4   | JBOD-1-5  | WD-WCAVY0114154 |
| 01   | 1/6  | da5   | JBOD-1-6  | WD-WMC5C0D9L6HV |
| 02   | 1/7  | da6   | JBOD-1-7  | WD-WCC6N5UY8H5P |
| 03   | 1/8  | da7   | JBOD-1-8  | WD-WCC300759632 |
| 30   | 1/9  | da8   | JBOD-1-9  | WD-WCC6N6DDJ7DT |
| 31   | 1/10 | da9   | JBOD-1/10 | WD-WCC6N6VTE2NF |
| 32   | 1/11 | da10  | JBOD-1/11 | WD-WMC5C0D8Z7FV |
| 33   | 1/12 | da11  | JBOD-1/12 | WD-WMC6N0J6S9AV |
| 10   | 1/13 | da12  | JBOD-1/13 | WD-WCC4MLULA4S4 |
| 11   | 1/14 | da13  | JBOD-1/14 | WD-WMC6N0F8FU0U |
| 12   | 1/15 | da14  | JBOD-1/15 | WD-WCAVY0090692 |
| 13   | 1/16 | da15  | JBOD-1/16 | WD-WCC6N5CLHYSS |

* da1 MK0171YFKMA4AG replaced 2022.05.08
* da12 MK0171YFKMA59G replaced 2022.04.12
* da8 WD-WCAVY0111166 replaced 2021.11.22
* da10 WD-WCAVY0127426 replaced 2016.09.15
* da1 S2F06GX5  replaced 2016.01.2?
* da2 WD-WCAVY0112831 replaced 2014.05.12
* da5 WD-WCAVY0107135 replaced 2017.03.25
* da13 W1E0B4NJ replaced 2017.06.xx
* da6 WD-WCAVY0127865 replaced 2018.01.07
* da6 WD-WMC6N0H8K48M replaced 2021.01.16
* da9 WD-WCAVY0117958 replaced 2021.03.15
* da15 WD-WCC4M5VJ4UK3 replaced 2021.06.18
* da9 WD-WMAY04440674 replaced 2021.08.27

## DEAD dfw0.psg.com

dfw0 drives `for i in 4 5 6 7; do echo /dev/ad$i; smartctl -a /dev/ad$i | egrep 'Model|Serial'; done`

|      |                    |              |      |
| ---- | ------------------ | ------------ | ---- |
| Bay  | Model              | Serial       |      |
|      |                    |              |      |
| ada0 | ST31000340NS       | 9QJ3Q29E     | 1TB  |
| ada1 | WD20EADS-00R6B0    | WCAVY0388932 | 2TB  |
| ada2 | WD2005FBYZ-01YCBB1 | WMC6N0F2KZU6 | 2TB  |
| ada3 | ST31000340NS       | 9QJ3M5N4     | 1TB  |
|      |                    |              |      |

dfw0 disk drive physical order

| ada4 | ada6 | ada5 | ada7 |
| ---- | ---- | ---- | ---- |
| ada0 | ada2 | ada1 | ada3 |

logical drive labels

| label/disk00 | ada0s3 |
| ------------ | ------ |
| label/disk01 | ada1s3 |
| label/disk02 | ada2s1 |
| label/disk03 | ada3s1 |

## DEAD nfs0.dfw.rg.net

### MoBo
* [PDSME+](http://www.supermicro.com/products/motherboard/Xeon3000/3010/PDSME_.cfm)
* [​AOC-SIM1U+ IPMI Card](http://www.supermicro.com/products/accessories/addon/SIM.cfm)

### DEAD nfs0.dfw.rg.net Disk Drives
```
for i in 0 1 2 3 4 5 6 7; do tw_cli /c2/p$i show serial; done
```

| Port     | Model              | Serial          | Size | Date               |
| -------- | ------------------ | --------------- | ---- | ------------------ |
| p0       | ST4000DM000-1F2168 | Z300L98C        | 4TB  | don't know         |
| p1       | WD4000F9YZ-09N20L1 | WD-WCC5D1DS4012 | 4TB  | 2019.04.07         |
| p2       | WD60EFRX-68L0BN1   | WD-WX41DA57H7UJ | 6TB  | 2018.03.09         |
| p3       | WD4000F9YZ-09N20L1 | WD-WCC5D2KHHYE8 | 4TB  | 2016.06.09         |
| p4       | ST4000DM000-1F2168 | Z300KBMM        | 4TB  | don't know         |
| p5       | ST4000DM000-1F2168 | Z300KBQN        | 4TB  | don't know         |
| p6       | ST4000DM000-1F2168 | Z300L8J5        | 4TB  | don't know         |
| p7       | WD4000F9YZ-09N20L1 | WD-WMC5D0D7V0L9 | 4TB  | 2015.12.13         |
|          |                    |                 |      |                    |
| p1       | ST4000DM000-1F2168 | Z300FKES        | 4TB  | removed 2019.04.07 |
| p2       | ST4000DM000-1F2168 | Z300L9T3        | 4TB  | removed 2018.03.09 |
| incoming | HUS724040ALS640    | PBK4K70X        | 4TB  | 2015.12.18         |

### Physical Drive layout

|      |      |      |      |
| ---- | ---- | ---- | ---- |
| 4    | 5    | 6    | 7    |
| 0    | 1    | 2    | 3    |

---
2022.08.07
